Wireless Optical Mouse Manual

Introduction Installation Wireless optical mouse function Setting program Troubleshooting

About This Manual

This manual is designed to assist you in installing and using the Wireless Mouse. Information in this document has been carefully checked for accuracy; however, no guarantee is given to the correctness of the contents. The information in this document is subject to change without notice.

Edition

1st Edition,

Copyright

© Copyright 2002

This document contains proprietary information protected by copyright. All rights are reserved. No part of this manual may be reproduced by any mechanical, electronic or other means, in any form, without prior written permission of the manufacturer.

Trademarks

All trademarks and registered trademarks are the property of their respective owners.

Federal Communications Commission Statement

This Equipment has been tested and found to comply with the limits for a class B digital device, pursuant to Part 15 of the Federal Communications Commission (FCC) rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation. This equipment generates, uses, and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation. If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

¨ Reorient or relocate the receiving antenna.

¨ Increase the separation between the equipment and receiver.

¨ Connect the equipment into and outlet on a circuit different from that to which the receiver is connected.

¨ Consult the dealer or an experienced radio/TV technician for help.

Warning

A shielded‑type power cord is required in order to meet FCC emission limits and to prevent interference to nearby radio and television reception. It is essential that only the supplied power cord be used.

Use only shielded cables to connect I/O devices to this equipment.

You are cautioned that changes or modifications not expressly approved by the party responsible for compliance could void your authority to operate the equipment.

1. INTRODUCTION

Thank you for purchasing the WIRELESS OPTICAL MOUSE. This User’s Manual contains information that will help you to operate your mouse as well as answer questions about certain special keys and buttons. Please keep this manual and the Setup CD in a safe place for future reference.

2. System Requirements

Before installing the Optical Mouse software, please make sure that the following hardware and software components are installed and correctly set up. The following system specifications are required:

· Pentium 133 or higher processor.

· Microsoft Windows® 98/ME/2000/XP operating system or later.

· Microsoft Internet Explorer 4.0 or later.

· 32MB of RAM, 64MB of RAM is recommended.

· CD-ROM or DVD drive.

· Two A3 alkaline batteries.

· To use the new enhanced Office features, you also need:

● Microsoft Office 97 or later is recommended. (With Word, Excel, Power Point or MS Outlook installed, the wireless optical mouse will perform more functions).

● The enhanced Office features are compatible with a number of other leading applications as well. (If the application function name is the same as the Hot Key printed name, pressing that Hot Key should perform the same function).

3. Installation

Package Contents: Batteries; Receiver; Software; mouse

Install the batteries in the mouse.

Turn off the computer. Connect the receiver to the desktop.

Turn on your PC, and then install the software.

### Installation for Windows® 98/ME/2000/XP

1. Before installing the Wireless Optical Mouse driver, check to see if there are any other mouse drivers already installed on your system. All other mouse drivers must be uninstalled BEFORE installing the Wireless Optical Mouse drivers.

2. Insert the Driver CD into your CD-ROM drive and the CD will Auto Run. If it does not, please choose (Run) from the Start Menu. The file name on the CD is ”AUTORUN”. The first screen is an introduction. Read it before proceeding to the next step. The software will automatically begin to install to your hard disk in a sub-directory titled C:\PROGRAM FILES\MAGIC FUNCTION\. After installation, you will be prompted to restart your computer in order to enable the Wireless Optical Mouse software.

3. Click (Finish) and restart your computer. The Wireless Optical Mouse Icon will be activated automatically after Windows restarts.

NOTE: After installing the Wireless Optical Mouse drivers, you must restart your computer, or the Wireless Optical Mouse software will not be enabled.

### Un-installation

To remove the Wireless Optical Mouse drivers from your system, simply go to Starting à Program Files à MAGIC FUNCTION and choose “Uninstall Magic Function Program” application software.

4. Wireless optical Mouse Functions

An Optical Mouse Function icon will be shown in system tray after Magic Function has been installed. Appears "Optical Mouse" as the Hint when mouse comes over it.A Pop-up Menu will appear with a mouse right-clicking of Optical Mouse icon in system tray.

The Pop-up Menu contains:

◆ Option: To bring up the options dialog box for you to program Mouse AP.

◆ Show/Hide Optical Mouse Icon: Show/Hide Optical Mouse Icon and the default setting is "Show"

◆ Help: Launch Help file of Magic function.

◆ About: Information about the driver

◆ Exit: Exit “Magic function” program

Magic Function Configuration:

◆ The Magic Function configuration tool will be located in the "Mouse Properties" from the MS "Control Panel"

5. Setting Wireless optical mouse and Program

Setting Wireless Optical Mouse:

◆ Make sure the receiver cable (purple) is plugged into the PS/2 keyboard port and the other cable (green) is plugged into the PS/2 mouse port.

◆ Establish communication between the receiver and mouse. The bottom of the receiver has two-channel switch. One is for keyboard and the other is for mouse. The bottom of the mouse also has a channel switch. When receiver’s mouse switch setting on CH2, then the mouse’s channel switch should be setting on CH2.

◆ The bottom of the receiver and mouse both has an ID setting button. Press the ID button on the receiver first; then the receiver’s LED will glitter (about 0.5 second glitter one time). Then press the ID button under the mouse. The receiver’s LED will stop glitter; it means the mouse’s setting up is completed.

◆ This type of wireless optical mouse can work in two radio frequency channels. You may need to switch channel, for example, if the signal from your mouse is conflicting with that from other users close by. To change channel, please refer to Step 2.

Setting Program:

This section describes how to use the Wireless Optical Mouse setting program. Once the software installation for the Wireless Optical Mouse is completed, the icon

is shown on the Windows Ò taskbar. Right click on the (Optical Mouse Icon) to activate a menu with options to configure the Magic Function Software.

5-1Magic Function: Configuration tool provided for you to design the mouse functions.

5-2 Mouse Buttons: There are 4 buttons of Magic function for Wireless Optical Mouse. And you can select the functionality of these buttons.

5-3 Function Assignment: There are totally 27 functionalities listed as the following and you can select one of them easily in this drop-pop menu.

1.Calculator | 2.Copy | 3.Copy/Paste
4.Control Panel | 5.Cut | 6.Display Property
7.Dos Shell | 8.Eject | 9.Email
10.Enter | 11.File Explorer | 12.F1-F12
13.Media Wheel | 14.My Document | 15. My Shortcut
16.Next Track | 17.Paste | 18.Play/Pause
19.Previous Track | 20.Property | 21.Screen Saver
22.Stop | 23.Switch Window | 24.System Property
25.Undo | 26.Volume Control | 27.WWW

5-4 Load Default Setting: Easily for you to get the Default Setting of Media Wheel

For My Shortcut functionality:

When you select this functionality, the dialog, as the following will pop-up.

By clicking the browse button , end-user can select an execution file to be launched by the assigned button.

After you assigned the shortcut, below dialog box will appear to indicate you that Shortcut location you selected.

### Magic Function

The below Interface will pup-up when you assign the button function as "Magic Function".

A-1 & A-3: Tack function. You can enable or disable it to make Magic Function UI to appear on the screen or disappear when mouse move away.

A-2: To close the Magic Function.

● The Media Wheel UI will come with function Hint in the central and change the color when you move mouse over the UI.

● The 10 functions of Magic Function includes:

1-5 ： 5-fix functions for Internet control functions, such as Home, Stop, Refresh, Back and Forward.

P1-P5 ： 5 programmable functions for you to define easily.

And the default functionality of P1-P5 is as the following:

P1: Launch the application of E-mail

P2: Launch File Explorer

P3: Open Control panel

P4: Open My document

P5: Open the Help file of Optical Mouse

Right-click the button of UI to bring the Magic Function setting dialog box.

6. Troubleshooting

If you have any problems using the Wireless Optical Mouse, please consult the Troubleshooting Guide below to see if your problem is listed.

Wireless Product Does Not Work

· Make sure you have connected the receiver correctly (please refer the setting up a wireless optical mouse). For optimal performance, place the receiver at least 8 inches or 20 centimeters away from other electrical devices, such as the computer, the computer monitor, or external storage drives.

· Make sure you have installed the batteries correctly. Check to make sure the batteries you have installed are not dead. Try the batteries in another device.

· If you are working on a metallic surface, try moving the receiver closer to the mouse or standing the receiver on its side.

· Try unplugging then reconnecting the receiver cable to the computer.

Wireless Product Is Not Detected

· Make sure the receiver cable (purple) is plugged into the PS/2 keyboard port and the other cable (green) is plugged into the PS/2 mouse port .Do not plug or unplug the receiver cable while the computer is running.

· In Windows you may have other system devices that conflict with the mouse, trackball, or keyboard. Check the IRQ/address settings of these devices for conflicts, and change the settings as required. Refer to your computer documentation to make these changes.

· Try unplugging then reconnecting the receiver cable to the computer.

Non-Wireless Pointing Device Is Not Detected

· Make sure the mouse cable is plugged into the right port - PS/2.

· In Windows you may have other system devices (e.g., a modem card) that conflict with the mouse. Check the IRQ/address settings of these devices for conflicts, and change the settings as required. If the problem persists, please contact technical support.

Screen Cursor Does Not Move Properly

For wireless devices, try changing the position of the receiver. It is possible that the receiver may be too far from the mouse. Or the computer monitor (or a large metal object) may be interfering with the receiver's radio reception. Also, the batteries may be low. Check the batteries as described previously. You may also need to re-establish the connection between the mouse and its receiver. To do this, first press the Channel button on the receiver, and then press the Channel button on the bottom of the mouse.

If you are using a mouse with optical technology and your tabletop surface is red in color or is highly reflective like a mirror, your tabletop surface may be interfering with the optical sensor of the mouse. Try using a traditional mouse pad, or use the mouse on a different tabletop surface.

I cannot properly install other software applications.

If you want to install another software application but experience problems, you may have to remove the Optical Mouse driver from your system memory. Right-click on the (Optical Mouse icon) and then chooses EXIT. Now install the desired software application. After completion of the new application software installation, restart your system, the Optical Mouse Icon will display in tray again.

**If you still cannot solve your problem, please contact with your local dealer. **